192.168.123.132 = 11000000. 10101000. 01111011. 10000100.

192:2=96+0

96:2=48+0

48:2=24+0

24:2=12+0

12:2=6+0

6:2=3+0

3:2=1+1

1:2=0+1

1 1 0 0 0 0 0 0

27 + 26 + 25 + 24 + 23 + 22 + 21 + 20 = 192

192.168.123. Network

.132 Host

-or-

192.168.123.0 - network address.

0.0.0.132 - host address.

PODMREŽA

255.255.255.0. = 11111111.11111111.11111111.0000000

11000000.10101000.01111011.10000100 -- IP address (192.168.123.132)

11111111.11111111.11111111.00000000 -- Subnet mask (255.255.255.0)

11000000.10101000.01111011.00000000 -- Network address (192.168.123.0) 00000000.00000000.00000000.10000100 -- Host address (000.000.000.132)

Class A: 255.0.0.0

Class B: 255.255.0.0

Class C: 255.255.255.0

* Class A networks use a default subnet mask of 255.0.0.0 and have 0-127 as their first octet. The address 10.52.36.11 is a class A address. Its first octet is 10, which is between 1 and 126, inclusive.
* Class B networks use a default subnet mask of 255.255.0.0 and have 128-191 as their first octet. The address 172.16.52.63 is a class B address. Its first octet is 172, which is between 128 and 191, inclusive.
* Class C networks use a default subnet mask of 255.255.255.0 and have 192-223 as their first octet. The address 192.168.123.132 is a class C address. Its first octet is 192, which is between 192 and 223, inclusive.

An IP address on a Class A network that has not been subnetted would have an address/mask pair similar to: 8.20.15.1 255.0.0.0. To see how the mask helps you identify the network and node parts of the address, convert the address and mask to binary numbers.

8.20.15.1 = 00001000.00010100.00001111.00000001

255.0.0.0 = 11111111.00000000.00000000.00000000

Once you have the address and the mask represented in binary, then identifying the network and host ID is easier. Any address bits which have corresponding mask bits set to 1 represent the network ID. Any address bits that have corresponding mask bits set to 0 represent the node ID.

8.20.15.1 = 00001000.00010100.00001111.00000001

255.0.0.0 = 11111111.00000000.00000000.00000000

-----------------------------------

net id | host id

netid = 00001000 = 8

hostid = 00010100.00001111.00000001 = 20.15.1

**Understanding Subnetting**

Subnetting allows you to create multiple logical networks that exist within a single Class A, B, or C network. If you do not subnet, you are only able to use one network from your Class A, B, or C network, which is unrealistic.

Each data link on a network must have a unique network ID, with every node on that link being a member of the same network. If you break a major network (Class A, B, or C) into smaller subnetworks, it allows you to create a network of interconnecting subnetworks. Each data link on this network would then have a unique network/subnetwork ID. Any device, or gateway, connecting *n* networks/subnetworks has *n* distinct IP addresses, one for each network / subnetwork that it interconnects.

In order to subnet a network, extend the natural mask using some of the bits from the host ID portion of the address to create a subnetwork ID. For example, given a Class C network of 204.17.5.0 which has a natural mask of 255.255.255.0, you can create subnets in this manner:

204.17.5.0 - 11001100.00010001.00000101.00000000

255.255.255.224 - 11111111.11111111.11111111.11100000

--------------------------|sub|----

By extending the mask to be 255.255.255.224, you have taken three bits (indicated by "sub") from the original host portion of the address and used them to make subnets. With these three bits, it is possible to create eight subnets. With the remaining five host ID bits, each subnet can have up to 32 host addresses, 30 of which can actually be assigned to a device *since host ids of all zeros or all ones are not allowed* (it is very important to remember this). So, with this in mind, these subnets have been created.

204.17.5.0 255.255.255.224 host address range 1 to 30

204.17.5.32 255.255.255.224 host address range 33 to 62

204.17.5.64 255.255.255.224 host address range 65 to 94

204.17.5.96 255.255.255.224 host address range 97 to 126

204.17.5.128 255.255.255.224 host address range 129 to 158

204.17.5.160 255.255.255.224 host address range 161 to 190

204.17.5.192 255.255.255.224 host address range 193 to 222

204.17.5.224 255.255.255.224 host address range 225 to 254

**Note:**There are two ways to denote these masks. First, since you are using three bits more than the "natural" Class C mask, you can denote these addresses as having a 3-bit subnet mask. Or, secondly, the mask of 255.255.255.224 can also be denoted as /27 as there are 27 bits that are set in the mask. This second method is used with [CIDR](http://www.cisco.com/c/en/us/support/docs/ip/routing-information-protocol-rip/13788-3.html#cidr). With this method, one of these networks can be described with the notation prefix/length. For example, 204.17.5.32/27 denotes the network 204.17.5.32 255.255.255.224. When appropriate the prefix/length notation is used to denote the mask throughout the rest of this document.

The network subnetting scheme in this section allows for eight subnets, and the network might appear as: